Redstar

If reply data is **0x12, 0x57**

This the final data, user get

Send fuel function, send read price, and send read total and then MQTT final response

Please note to pump status = fuel

If reply data is 0x12, 0x77

This the pump approve sending